

**Report Common Assignment: Parallel Tarjan**

**Lecturer: Francesco Moscato - fmoscato@unisa.it**

* **Marcone Giuseppe - 0622701896 – g.marcone2@studenti.unisa.it**
* **Pizzulo Rocco Gerardo - 0622701990 – r.pizzulo@studenti.unisa.it**
* **Russo Luigi - 0622702071 – l.russo86@studenti.unisa.it**



# Index

[Index 2](#_Toc1)

[Problem description 3](#_Toc2)

[Solution 3](#_Toc3)

[Experimental setup 4](#_Toc4)

[Hardware 4](#_Toc5)

[Memory Device 5](#_Toc6)

[Software 6](#_Toc7)

[Performance, SpeedUp & Efficiency 6](#_Toc8)

[Case study 1: send without pack 6](#_Toc9)

[6000-150 6](#_Toc10)

[6000-250 7](#_Toc11)

[6000-400 7](#_Toc12)

[Case study 2: send with pack 7](#_Toc13)

[6000-150 7](#_Toc14)

[6000-250 7](#_Toc15)

[6000-400 7](#_Toc16)

[Final consideration 8](#_Toc17)

# Problem description

Provided a parallell version of the Tarjan's algorithm to find Strongly Connected Components in a Graph. The implementation is an hibrid  message passing / shared memory paradigm implemented by using MPI and openMP.

There are no constraints on the graph structure and allocation type.

# Solution

A version was implemented in which the graph is read from text files and divided into subgraphs each of which is sent to an MPI process.

After that a reduction mechanism was implemented; one half of the processes processes the partial graph and forwards the result to the others, the mechanism continues until the whole graph converges to process 0. MPI (Message Passing Interface) was used for communication between processes.

Two versions were provided for the parallel program with 2 different communication systems: in the first case, communication was via the functions MPI\_Send () and MPI\_Recv () by sending the fields separately, in the second case, data were sent after encapsulation via MPI\_Pack().

In addition, a second level of parallelization was added via OpenMP trying to make the loops more efficient.

Initially, measurements were made with MPI and later with the addition of OpenMP.

# Experimental setup

## Hardware

*Architecture: x86\_64*

*CPU op-mode(s): 32-bit, 64-bit*

*Address sizes: 39 bits physical, 48 bits virtual*

*Byte Order: Little Endian*

*CPU(s): 8*

*On-line CPU(s) list: 0-7*

*Vendor ID: GenuineIntel*

*Model name: Intel(R) Core(TM) i7-10510U CPU @ 1.80GHz*

*CPU family: 6*

*Model: 142*

*Thread(s) per core: 2*

*Core(s) per socket: 4*

*Socket(s): 1*

*Stepping: 12*

*CPU(s) scaling MHz: 39%*

*CPU max MHz: 4900.0000*

*CPU min MHz: 400.0000*

*BogoMIPS: 4599.93*

*Flags: fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush dts acpi mmx fxsr sse sse2 ss ht tm pbe syscall nx pdpe1gb rdtscp lm constant\_tsc art arch\_perfmon pebs bts rep\_good nopl xtopology n*

*onstop\_tsc cpuid aperfmperf pni pclmulqdq dtes64 monitor ds\_cpl vmx est tm2 ssse3 sdbg fma cx16 xtpr pdcm pcid sse4\_1 sse4\_2 x2apic movbe popcnt tsc\_deadline\_timer aes xsave avx f16c rdrand lahf\_lm abm 3dnowprefet*

*ch cpuid\_fault epb invpcid\_single ssbd ibrs ibpb stibp ibrs\_enhanced tpr\_shadow vnmi flexpriority ept vpid ept\_ad fsgsbase tsc\_adjust sgx bmi1 avx2 smep bmi2 erms invpcid mpx rdseed adx smap clflushopt intel\_pt xs*

*aveopt xsavec xgetbv1 xsaves dtherm ida arat pln pts hwp hwp\_notify hwp\_act\_window hwp\_epp md\_clear flush\_l1d arch\_capabilities*

## Memory Device

*Array Handle: 0x1000*

*Error Information Handle: Not Provided*

*Total Width: 64 bits*

*Data Width: 64 bits*

*Size: 8 GB*

*Form Factor: Row Of Chips*

*Set: None*

*Locator: MotherBoard*

*Bank Locator: BANK 0*

*Type: LPDDR3*

*Type Detail: Synchronous*

*Speed: 2133 MT/s*

*Manufacturer: Samsung*

*Serial Number: 55000000*

*Asset Tag: 01000000*

*Part Number: K4EBE304EC-EGCG*

*Rank: 2*

*Configured Memory Speed: 2133 MT/s*

*Minimum Voltage: Unknown*

*Maximum Voltage: Unknown*

*Configured Voltage: 1.2 V*

*Memory Technology: DRAM*

*Memory Operating Mode Capability: Volatile memory*

*Firmware Version: 55000000*

*Module Manufacturer ID: Bank 1, Hex 0xCE*

*Module Product ID: Unknown*

*Memory Subsystem Controller Manufacturer ID: Unknown*

*Memory Subsystem Controller Product ID: Unknown*

*Non-Volatile Size: None*

*Volatile Size: 8 GB*

*Cache Size: None*

*Logical Size: None*

## Software

*OS: Linux fedora 6.1.6-200.fc37.x86\_64*

*GCC: gcc (GCC) 12.2.1 20221121 (Red Hat 12.2.1-4)*

*Swap: 8GB*

# Performance, SpeedUp & Efficiency



## Case study 1: send without pack

In the first case study, communication was implemented by means of MPI\_send() and MPI\_Recv() without encapsulating the data, thus sending them separately.



Both sequential and parallel compilation were done with the -O3 gcc optimization and measurements were performed with 1, 2, 4 and 8 MPI processes and 4 OpenMP threads.

The graph used has 6000 vertices and 150 arcs for the first measurement, 250 for the second and 400 for the third

### 6000-150





### 6000-250



### 6000-400

Case study 2: send with pack





In the second case study, the submitted vertex fields were first encapsulated with MPI\_Pack() and only then submitted with MPI\_Send(), so the number of submissions was reduced by 1/3.



Again, this was compiled with the gcc -O3 option, measurements were performed with 1, 2, 4 and 8 MPI processes and 4 OpenMP threads.

The graph used has 6000 vertices and 150 arcs for the first measurement, 250 for the second and 400 for the third



### 6000-150



### 6000-250



### 6000-400



# Final consideration